NOTE: This as-constructed sanitary drainage plan has been prepared and supplied to Council by the licensed person responsible for the installation of the drainage. Council accepts no responsibility for variations in measurements or depths that may have occurred. The depth and location of any existing drainage shown should only be considered as an approximation. The Bundaberg Regional Council (and its councillors, officers, servants and agents) contract and agree to supply information only on that basis. Drainage layout diagrams are NOT TO SCALE legend	NEW SERVICE
BORE WATER	-------BW-------
IRRIGATION	--------IR--------
HOUSE DRAIN	--------HD--------
VENT	--------V--------
WATER	--------W--------
GENERAL
BOUNDARY	---- · ---- · ----
RETAINING WALL	XXXXXXXXXXX
ABBREVIATIONS
AAV	AIR ADMITTANCE VALVE
AR	ARTICULATION
B	BASIN
BID	BIDET
BTH	BATH
CWM	CLOTHES WASHING MACHINE
DG	DISCONNECTOR GULLY
FW	FLOOR WASTE GULLY
GIT	GREASE INTERCEPTOR TRAP
IO	INSPECTION OPENING
IOS	INSPECTION OPENING TO SURFACE
ISS	INSPECTION SHAFT TO SURFACE
JU	JUMP UP
LT	LAUNDRY TROUGH
ORG	OVERFLOW RELIEF GULLY
PCV	PRESSURE CONTROL VALVE
SAN	SANITARY DRAIN / PLUMBING
SHR	SHOWER
SK	SINK
SPA	SPA BATH
ST	STACK
TD	TUNDISH
VP	VENT PIPE
WC	WATER CLOSET
WM	WATER METER
WWTP	WASTE WATER TREATMENT PLANT
DRAWN	DATE	SHEET	REV.
Project Details Permit Number: 311-.………………………………….…………………. Address…………………………………………………………………………….. ………………………………………………………………………………….……… Lot and Plan Details…………………………………………………………… …………………………………………………………………………………………. as constructed
installed by Responsible Person…………………………………………………………….. Licence Number………………………………………………...……………….. Date…………………………………………………….………………………………